<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="34.44375" y2="0" width="0.254" layer="20"/>
<wire x1="34.44375" y1="0" x2="34.44375" y2="25.93625" width="0.254" layer="20"/>
<wire x1="34.44375" y1="25.93625" x2="0" y2="25.93625" width="0.254" layer="20"/>
<wire x1="0" y1="25.93625" x2="0" y2="0" width="0.254" layer="20"/>
<text>spider regulator</text>
<text>v1.2</text>
<text>-</text>
<text>+</text>
</plain>
<libraries>
<library name="coati">
<packages>
<package name="TT2D10">
</package>
<package name="0207/7">
</package>
<package name="TO220V+6237BG">
</package>
<package name="KOBICONN-5013">
</package>
<package name="KEYSTONE-593-594">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="coati" package="TT2D10" value="1000u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="coati" package="0207/7" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="coati" package="0207/7" value="1.2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="coati" package="TO220V+6237BG" value="LM317V">
<attribute name="NAME"/>
</element>
<element name="J1" library="coati" package="KOBICONN-5013" value="KOBICONN-5013">
<attribute name="NAME"/>
</element>
<element name="S1" library="coati" package="KEYSTONE-593-594" value="KEYSTONE-593-594">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="SHIELD"/>
<contactref element="S1" pad="F2"/>
<contactref element="S1" pad="F3"/>
<contactref element="S1" pad="F1"/>
<contactref element="R2" pad="2"/>
<contactref element="C1" pad="-"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="TIP"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="S1" pad="M2"/>
<contactref element="S1" pad="M3"/>
<contactref element="S1" pad="M1"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="+"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
