<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="45.5" x2="0" y2="7.5" width="0.254" layer="20"/>
<wire x1="7" y1="0" x2="110" y2="0" width="0.254" layer="20"/>
<wire x1="117" y1="7.5" x2="117" y2="45.5" width="0.254" layer="20"/>
<wire x1="110" y1="53" x2="7" y2="53" width="0.254" layer="20"/>
<wire x1="117" y1="45.5" x2="110" y2="45.5" width="0.254" layer="20"/>
<wire x1="110" y1="45.5" x2="110" y2="53" width="0.254" layer="20"/>
<wire x1="117" y1="7.5" x2="110" y2="7.5" width="0.254" layer="20"/>
<wire x1="110" y1="7.5" x2="110" y2="0" width="0.254" layer="20"/>
<wire x1="7" y1="53" x2="7" y2="45.5" width="0.254" layer="20"/>
<wire x1="7" y1="45.5" x2="0" y2="45.5" width="0.254" layer="20"/>
<wire x1="0" y1="7.5" x2="7" y2="7.5" width="0.254" layer="20"/>
<wire x1="7" y1="7.5" x2="7" y2="0" width="0.254" layer="20"/>
<text>extension 1.2</text>
<text>Input</text>
<text>Output</text>
<text>On/Off</text>
<text>Extension</text>
</plain>
<libraries>
<library name="coati">
<packages>
<package name="PJRAN2X1U">
</package>
<package name="LED5MM">
</package>
<package name="0207/7">
</package>
<package name="TT2D10">
</package>
<package name="C025-025X070">
</package>
<package name="RK11K">
</package>
<package name="0052-EVX">
</package>
<package name="TT2D5-MEDIUM">
</package>
<package name="20-1655">
</package>
<package name="DIL08">
</package>
<package name="TT2D6">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="H5" library="coati" package="20-1655" value="20-1655">
<attribute name="NAME"/>
</element>
<element name="H1" library="coati" package="20-1655" value="20-1655">
<attribute name="NAME"/>
</element>
<element name="R17" library="coati" package="0207/7" value="15R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="coati" package="0207/7" value="15R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H7" library="coati" package="20-1655" value="20-1655">
<attribute name="NAME"/>
</element>
<element name="H3" library="coati" package="20-1655" value="20-1655">
<attribute name="NAME"/>
</element>
<element name="R19" library="coati" package="0207/7" value="15R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="coati" package="0207/7" value="15R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H11" library="coati" package="20-1655" value="20-1655">
<attribute name="NAME"/>
</element>
<element name="H9" library="coati" package="20-1655" value="20-1655">
<attribute name="NAME"/>
</element>
<element name="R25" library="coati" package="0207/7" value="15R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="coati" package="0207/7" value="15R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H2" library="coati" package="20-1655" value="20-1655">
<attribute name="NAME"/>
</element>
<element name="H4" library="coati" package="20-1655" value="20-1655">
<attribute name="NAME"/>
</element>
<element name="R20" library="coati" package="0207/7" value="15R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="coati" package="0207/7" value="15R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H12" library="coati" package="20-1655" value="20-1655">
<attribute name="NAME"/>
</element>
<element name="R28" library="coati" package="0207/7" value="15R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H10" library="coati" package="20-1655" value="20-1655">
<attribute name="NAME"/>
</element>
<element name="R26" library="coati" package="0207/7" value="15R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H8" library="coati" package="20-1655" value="20-1655">
<attribute name="NAME"/>
</element>
<element name="R24" library="coati" package="0207/7" value="15R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H6" library="coati" package="20-1655" value="20-1655">
<attribute name="NAME"/>
</element>
<element name="R22" library="coati" package="0207/7" value="15R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="coati" package="C025-025X070" value="47n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="coati" package="0207/7" value="10R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="coati" package="TT2D6" value="220u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="coati" package="C025-025X070" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="coati" package="TT2D5-MEDIUM" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="coati" package="0207/7" value="1.2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="INPUT" library="coati" package="PJRAN2X1U" value="DUAL-RCA-PJRAN2X1U">
<attribute name="NAME"/>
</element>
<element name="OUTPUT" library="coati" package="PJRAN2X1U" value="DUAL-RCA-PJRAN2X1U">
<attribute name="NAME"/>
</element>
<element name="LED1" library="coati" package="LED5MM" value="LED5MM">
<attribute name="NAME"/>
</element>
<element name="R1" library="coati" package="0207/7" value="10K"/>
<element name="C1" library="coati" package="TT2D10" value="1000u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="coati" package="C025-025X070" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P1" library="coati" package="RK11K" value="RK11K">
<attribute name="NAME"/>
</element>
<element name="S1" library="coati" package="0052-EVX" value="0052-EVX">
<attribute name="NAME"/>
</element>
<element name="IC1" library="coati" package="DIL08" value="LM386">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="R10" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="H6" pad="1"/>
<contactref element="H12" pad="1"/>
<contactref element="H9" pad="1"/>
<contactref element="H3" pad="1"/>
<contactref element="R19" pad="1"/>
<contactref element="R19" pad="1"/>
<contactref element="R22" pad="1"/>
<contactref element="R22" pad="1"/>
<contactref element="R25" pad="1"/>
<contactref element="R25" pad="1"/>
<contactref element="R28" pad="1"/>
<contactref element="R28" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="INPUT" pad="SLEEVE1"/>
<contactref element="INPUT" pad="SLEEVE2"/>
<contactref element="OUTPUT" pad="SLEEVE2"/>
<contactref element="OUTPUT" pad="SLEEVE1"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="1"/>
<contactref element="P1" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="N$32">
<contactref element="H5" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="H6" pad="2"/>
<contactref element="H6" pad="3"/>
<contactref element="R22" pad="2"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="N$36">
<contactref element="H7" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="H8" pad="2"/>
<contactref element="H8" pad="3"/>
<contactref element="R24" pad="2"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="N$41">
<contactref element="H11" pad="1"/>
<contactref element="R27" pad="1"/>
<contactref element="R27" pad="1"/>
<contactref element="H12" pad="2"/>
<contactref element="H12" pad="3"/>
<contactref element="R28" pad="2"/>
<contactref element="R28" pad="2"/>
</signal>
<signal name="N$46">
<contactref element="H2" pad="1"/>
<contactref element="R18" pad="1"/>
<contactref element="R18" pad="1"/>
<contactref element="H3" pad="3"/>
<contactref element="H3" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="N$63">
<contactref element="H4" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="H5" pad="3"/>
<contactref element="H5" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="N$69">
<contactref element="H8" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="H9" pad="2"/>
<contactref element="H9" pad="3"/>
<contactref element="R25" pad="2"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="N$98">
<contactref element="H10" pad="1"/>
<contactref element="R26" pad="1"/>
<contactref element="R26" pad="1"/>
<contactref element="H11" pad="3"/>
<contactref element="H11" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="N$102">
<contactref element="H1" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="H2" pad="2"/>
<contactref element="H2" pad="3"/>
<contactref element="R18" pad="2"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="C3" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="+"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="C3" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="H7" pad="3"/>
<contactref element="R26" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="H10" pad="2"/>
<contactref element="H10" pad="3"/>
<contactref element="R17" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="H1" pad="2"/>
<contactref element="H1" pad="3"/>
<contactref element="C4" pad="-"/>
<contactref element="R20" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="H4" pad="2"/>
<contactref element="H4" pad="3"/>
<contactref element="R23" pad="2"/>
<contactref element="R23" pad="2"/>
<contactref element="H7" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R9" pad="2"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="C10" pad="-"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$17">
<contactref element="R9" pad="1"/>
<contactref element="C10" pad="+"/>
</signal>
<signal name="N$34">
<contactref element="C5" pad="2"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="S$1">
</signal>
<signal name="VCC">
<contactref element="LED1" pad="A"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="+"/>
<contactref element="S1" pad="3"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="LED1" pad="K"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="INPUT" pad="TIP1"/>
<contactref element="OUTPUT" pad="TIP1"/>
<contactref element="INPUT" pad="SHUNT1"/>
<contactref element="OUTPUT" pad="SHUNT1"/>
<contactref element="P1" pad="3"/>
</signal>
<signal name="N$7">
</signal>
<signal name="N$9">
<contactref element="OUTPUT" pad="TIP2"/>
<contactref element="INPUT" pad="TIP2"/>
<contactref element="S1" pad="2"/>
<contactref element="OUTPUT" pad="SHUNT2"/>
<contactref element="INPUT" pad="SHUNT2"/>
</signal>
<signal name="N$6">
<contactref element="P1" pad="2"/>
<contactref element="IC1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
